WPDT
16.0

Problem
{
    Type  EM
    Coordinate  Cartesian
}

Material
{
    Air {
        Color  205 205 205  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Magnetic-Property {
            Permeability  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
    PEC {
        Color  230 230 25  // R,G,B
        Type  PEC
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
    bkg45 {
        Color  0 255 0  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  "4.5"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Magnetic-Property {
            Permeability  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
    bkg200 {
        Color  0 0 255  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  "20"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Magnetic-Property {
            Permeability  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
    bkg350 {
        Color  128 128 255  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  "35"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Magnetic-Property {
            Permeability  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
    dummy_m65_3 {
        Color  255 128 0  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  "65"
            Conductivity  "3"
            Loss-Tangent  "0"
        }
        Magnetic-Property {
            Permeability  "1"
            Conductivity  "0"
            Loss-Tangent  "0"
        }
        Mass {
            Density    "1000"
            Velocity-P "1500"
            Velocity-S "0"
        }
    }
}

Project
{
    Unit {
        Length     meter  // (m)
        Time       second  // (s)
        Frequency  hertz  // (Hz)
        Input-Frequency  Frequency
    }
    Background {
        Homogeneous {
            Material  bkg45
        }
    }
    Boundary {
        Xmin  Open-at-input-position  "-0.015"
        Xmax  Open-at-input-position  "0.135"
        Ymin  Open-at-input-position  "-0.015"
        Ymax  Open-at-input-position  "0.195"
        Zmin  Open-at-input-position  "-0.015"
        Zmax  Open-at-input-position  "0.1425"
    }
    Frequency {
        Freq-Range {
            Fmin  "3e7"  // Frequency unit is defined at "Unit item"
            Fmax  "3e9"
        }
        Default-Pulse
        /* the default pulse .........
        BHW {
            Amplitude  "1"
            Delay      "0"
            Order      "1"
            Frequency  "895255147.7"
        }
        ........................... */
    }
    Mesh {
        Manual {
            Grid  "110"  "140"  "105"
            Ctrl-Point  0
        }
        Uniform_layer_test {
               X 0
               Y 0
               Z 0
        }
        Option {
            MinMax-Ratio  "0.001"
            Adjust-Ratio  "1.3"
        }
        Solid {
            Min-Angle  "3"
        }
    }
    Cylindrical_Mesh {
        Automatic {
            PPW  10  10  10  
            MinMax-Ratio  0.01
            Adjust-Ratio  1.3
            R-Phi  0.55
        }
        Misc {
			Rmin 0.1
			Rmax 1
			Zmin -1
			Zmax 1
			Phimin -3.14159
			Phimax 3.14159
			Triangle_min_angle 3
        }
        Boundary_Conditions {
			R 1 1
			Phi 1 1
			Z 1 1
        }
    }
    Time {
        Time-Step {
            Automatic
        }
        Time-Window {
            User-defined  "2e-008"
        }
        Tolerance {
            Decay      -80  // (dB)
            Variation  -80  // (dB)
        }
        Recording-Interval {
            Observer  "10"
            Snapshot  "5"
        }
    }
    Method {
        Solver  AUTO
        ADI-PPP  20  // Points Per Period
    }
}

Source
{
    Source1 {
        Type {
            Dipole Electric
            Position  "0.045"  "0.045"  "-0.002"
            Polarization  "0"  "0"  "1"  // Hx,Hy,Hz
        }
        Excitation {
            Amplitude  "1"
            Delay  "0"
            Project-Pulse
        }
    }
}

Snapshot
{
    Face {
        x_fs_1 {
            Onwer-Name  NULL
            Component  7
            Face-ID  0
            Lower-Point   "0.06"  "-0.015"  "-0.015"
            Higher-Point  "0.06"  "0.195"  "0.1425"
            Normal  0
            Mesh-Type 2
            Mesh-Density 5
            Post    0
        }
        y_fs_1 {
            Onwer-Name  NULL
            Component  7
            Face-ID  0
            Lower-Point   "-0.015"  "0.1"  "-0.015"
            Higher-Point  "0.135"  "0.1"  "0.1425"
            Normal  1
            Mesh-Type 2
            Mesh-Density 5
            Post    0
        }
        z_fs_1 {
            Onwer-Name  NULL
            Component  7
            Face-ID  0
            Lower-Point   "-0.015"  "-0.015"  "0.05"
            Higher-Point  "0.135"  "0.195"  "0.05"
            Normal  2
            Mesh-Type 2
            Mesh-Density 5
            Post    0
        }
    }
}

Voxel
{
    breast {
        LCS_Origin 0 0 0
        LCS_U_AXIS 1 0 0
        LCS_V_AXIS 0 1 0
        Resolution 0.0015 0.0015 0.0015
        Unit meter
        Load_Position 0 0 0
        Volume_Usage_Type 0
        Permittivity Load
        Electric_Conductivity Load
        Permeability Bulk 1
        Magnetic_Conductivity Bulk 0
       }
}

Multi-Domain
{
    Enable
    Input-Method  Position
    Num-Div  1 1 1
    X-Pos { }
    Y-Pos { }
    Z-Pos { }
    Subdomain_solver_type { 0 }
}

Hybrid-Domain
{
    Disable
    Background {
        Type  ECT
        Box   0 0 0   0 0 0
    }
}

Option
{
    Observer-Spectrum  1
    ResultType-ParamAnal 0
    Warning-Message-Level 0
    Index-Ref-Pulse 2
}

Comparison-Data
{
}

Parametric-Analysis
{
    Include-Default-Set  No
}

Result-Enable
{
    Source {
        Transient 1
        Spectrum  1
    }
    Observer {
        Transient 1
        Spectrum  1
    }
    Lumped-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  1
        Incident-Voltage-Spectrum   1
        Incident-Current-Transient  1
        Incident-Current-Spectrum   1
        Scattered-Voltage-Transient 1
        Scattered-Voltage-Spectrum  1
        Scattered-Current-Transient 1
        Scattered-Current-Spectrum  1
    }
    Wave-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  1
        Incident-Voltage-Spectrum   1
        Incident-Current-Transient  1
        Incident-Current-Spectrum   1
        Scattered-Voltage-Transient 1
        Scattered-Voltage-Spectrum  1
        Scattered-Current-Transient 1
        Scattered-Current-Spectrum  1
    }
    Spice {
        Voltage-Transient  1
        Voltage-Spectrum   1
        Current-Transient  1
        Current-Spectrum   1
    }
    RLCD {
        Voltage-Transient  1
        Voltage-Spectrum   1
        Current-Transient  1
        Current-Spectrum   1
    }
    Snapshot {
        Enable  1
    }
    Far-Field {
        Enable  1
    }
}

Variable-Sub-System
{
}

Name-System
{
    Body  {
        Name  Body
        Index 2
    }
    Body-Copy  {
        Name  c
        Index 1
    }
    Body-Mirror  {
        Name  m
        Index 1
    }
    Body-Rotate  {
        Name  r
        Index 1
    }
    Body-Trans  {
        Name  t
        Index 1
    }
}

Extension-Data
{
      FaceSnapshot-Mesh-by-Center     0
}

Water-Mark
{
{000041-018467-006334-026500}
}

