WPDT
10005.2

Problem
{
    Type  EM
    Coordinate  Cartesian
}

Material
{
    Air {
        Color  205 205 205  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  1
            Conductivity  0
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  1
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    1.204
            Velocity-P 343
            Velocity-S 0
        }
    }
    PEC {
        Color  230 230 25  // R,G,B
        Type  PEC
        Mass {
            Density    1000
            Velocity-P 1500
            Velocity-S 0
        }
    }
    M1 {
        Color  225 200 175  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  2
            Conductivity  0
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  1
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    1000
            Velocity-P 1500
            Velocity-S 0
        }
    }
    M2 {
        Color  0 0 255  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  3
            Conductivity  10
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  1
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    1000
            Velocity-P 1500
            Velocity-S 0
        }
    }
}

Project
{
    Unit {
        Length     meter  // (m)
        Time       second  // (s)
        Frequency  hertz  // (Hz)
        Input-Frequency  Frequency
    }
    Background {
        Homogeneous {
            Material  Air
        }
    }
    Boundary {
        Xmin  Open-at-input-position  -0.1
        Xmax  Open-at-input-position  2.1
        Ymin  Open-at-input-position  -0.1
        Ymax  Open-at-input-position  1.1
        Zmin  Open-at-input-position  -0.1
        Zmax  Open-at-input-position  1.1
    }
    Frequency {
        Freq-Range {
            Fmin  1000000
            Fmax  100000000
        }
        Default-Pulse
        /* the default pulse .........
        BHW {
            Amplitude  1
            Delay      0
            Order      1
            Frequency  29841838.26
        }
        ........................... */
    }
    Mesh {
        Manual {
            Grid  44  24  24  
            Ctrl-Point  0
        }
        Uniform_layer_test {
               X 0
               Y 0
               Z 0
        }
        Solid {
            Min-Angle  3
        }
    }
    Cylindrical_Mesh {
        Automatic {
            PPW  10  10  10  
            MinMax-Ratio  0.01
            Adjust-Ratio  1.3
            R-Phi  0.55
        }
        Misc {
			Rmin 0.1
			Rmax 1
			Zmin -1
			Zmax 1
			Phimin -3.141592654
			Phimax 3.141592654
			Triangle_min_angle 3
        }
        Boundary_Conditions {
			R 1 1
			Phi 1 1
			Z 1 1
        }
    }
    Time {
        Time-Step {
            Delta-Time  1e-012
            Type  Automatic
        }
        Time-Window {
            End-Time  2.593372742e-007
            Type  Automatic
        }
        Tolerance {
            Decay      -40  // (dB)
            Variation  -30  // (dB)
        }
        Recording-Interval {
            Observer  20
            Snapshot  2
        }
    }
    Method {
        Solver  AUTO
        ADI-PPP  20  // Points Per Period
    }
}

Geometry_v2.0 
{
	[solids]
	[solid]
		Name: "Box1"
		Material: "M1"
		Mesh: "1"
		Name: "Box1"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape1"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "0, 0, 0"
		Corner2: "0.5, 1, 0.5"
		[end box]

		[end components]
	[end solid]

	[solid]
		Name: "Box2"
		Material: "M2"
		Mesh: "1"
		Name: "Box2"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape2"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "0.5, 0, 0"
		Corner2: "1, 1, 0.5"
		[end box]

		[end components]
	[end solid]

	[solid]
		Name: "Box3"
		Material: "PEC"
		Mesh: "1"
		Name: "Box3"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape3"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "1, 0, 0"
		Corner2: "2, 1, 0.5"
		[end box]

		[end components]
	[end solid]

	[solid]
		Name: "Box4"
		Material: "PEC"
		Mesh: "1"
		Name: "Box4"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape4"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "0, 0, 0.5"
		Corner2: "0.5, 1, 1"
		[end box]

		[end components]
	[end solid]

	[solid]
		Name: "Box5"
		Material: "Air"
		Mesh: "1"
		Name: "Box5"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape5"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "0.5, 0, 0.5"
		Corner2: "1, 1, 1"
		[end box]

		[end components]
	[end solid]

	[solid]
		Name: "Box6"
		Material: "PEC"
		Mesh: "1"
		Name: "Box6"
		Transparency: "0"
		[components]

		[box]
		Operation Type: "add"
		Name: "Shape6"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Corner1: "1, 0, 0.5"
		Corner2: "2, 1, 1"
		[end box]

		[end components]
	[end solid]

	[end solids]


}

Source
{
    Source1 {
        Type {
            Dipole Electric
            Position  0  0  0  // x,y,z
            Polarization  0  0  1  // Hx,Hy,Hz
        }
        Excitation {
            Amplitude  1
            Delay  0
            Project-Pulse
        }
    }
}

Observer
{
    Obs1 {
        Component  7
        Position  0.75  0  0.2  // x,y,z
    }
    Obs2 {
        Component  7
        Position  0.75  0.5  0.5  // x,y,z
    }
    Obs3 {
        Component  7
        Position  0.75  1  0.75  // x,y,z
    }
}

Multi-Domain
{
    Enable
    Input-Method  Position
    Num-Div  1 1 1
    X-Pos { }
    Y-Pos { }
    Z-Pos { }
    Subdomain_solver_type { 0 }
}

Hybrid-Domain
{
    Disable
    Background {
        Type  ECT
        Box   0 0 0   0 0 0
    }
}

Option
{
    Observer-Spectrum  1
    ResultType-ParamAnal 0
}

Comparison-Data
{
}

Parametric-Analysis
{
}

Result-Enable
{
    Source {
        Transient 1
        Spectrum  1
    }
    Observer {
        Transient 1
        Spectrum  1
    }
    Lumped-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  0
        Incident-Voltage-Spectrum   0
        Incident-Current-Transient  0
        Incident-Current-Spectrum   0
        Scattered-Voltage-Transient 0
        Scattered-Voltage-Spectrum  0
        Scattered-Current-Transient 0
        Scattered-Current-Spectrum  0
    }
    Wave-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  0
        Incident-Voltage-Spectrum   0
        Incident-Current-Transient  0
        Incident-Current-Spectrum   0
        Scattered-Voltage-Transient 0
        Scattered-Voltage-Spectrum  0
        Scattered-Current-Transient 0
        Scattered-Current-Spectrum  0
    }
    Spice {
        Voltage-Transient  1
        Voltage-Spectrum   0
        Current-Transient  1
        Current-Spectrum   0
    }
    RLCD {
        Voltage-Transient  1
        Voltage-Spectrum   0
        Current-Transient  1
        Current-Spectrum   0
    }
    Snapshot {
        Enable  0
    }
    Far-Field {
        Enable  0
    }
}

Variable-Sub-System
{
}

Name-System
{
    Body  {
        Name  Body
        Index 1
    }
    Body-Copy  {
        Name  c
        Index 1
    }
    Body-Mirror  {
        Name  m
        Index 1
    }
    Body-Rotate  {
        Name  r
        Index 1
    }
    Body-Trans  {
        Name  t
        Index 1
    }
}

Water-Mark
{
{019718-019895-005447-021726}
}

