WPDT
10005.2

Problem
{
    Type  EM
    Coordinate  Cartesian
}

Material
{
    Air {
        Color  205 205 205  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  1
            Conductivity  0
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  1
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    1.204
            Velocity-P 343
            Velocity-S 0
        }
    }
    PEC {
        Color  230 230 25  // R,G,B
        Type  PEC
        Mass {
            Density    0
            Velocity-P 0
            Velocity-S 0
        }
    }
    NormalMaterial2 {
        Color  225 200 175  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  2
            Conductivity  0
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  2
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    0
            Velocity-P 0
            Velocity-S 0
        }
    }
    NormalMaterial1 {
        Color  225 200 175  // R,G,B
        Type  Normal
        Electric-Property {
            Permittivity  4
            Conductivity  0
            Loss-Tangent  0
        }
        Magnetic-Property {
            Permeability  1
            Conductivity  0
            Loss-Tangent  0
        }
        Mass {
            Density    0
            Velocity-P 0
            Velocity-S 0
        }
    }
}

Project
{
    Unit {
        Length     meter  // (m)
        Time       second  // (s)
        Frequency  hertz  // (Hz)
        Input-Frequency  Frequency
        Domain {
            X  -8.4  8.4
            Y  -8.4  8.4
            Z  -8.4  8.4
        }
    }
    Background {
        Homogeneous {
            Material  NormalMaterial2
        }
    }
    Boundary {
        Xmin  Open-with-gap  -8.4
        Xmax  Open-with-gap  8.4
        Ymin  Open-with-gap  -8.4
        Ymax  Open-with-gap  8.4
        Zmin  Open-with-gap  -8.4
        Zmax  Open-with-gap  8.4
    }
    Frequency {
        Freq-Range {
            Fmin  45400.6
            Fmax  21619300
        }
        BHW {
            Amplitude  1
            Delay      0
            Order      1
            Frequency  6451610
        }
    }
    Mesh {
        Automatic {
            PPW  20  20  20  
            MinMax-Ratio  0.01
            Adjust-Ratio  1.25
            Ctrl-Point  0
        }
        Uniform_layer_test {
               X 0
               Y 0
               Z 0
        }
        Solid {
            Min-Angle  3
        }
    }
    Cylindrical_Mesh {
        Automatic {
            PPW  10  10  10  
            MinMax-Ratio  0.01
            Adjust-Ratio  1.3
            R-Phi  0.55
        }
        Misc {
			Rmin 0.1
			Rmax 1
			Zmin -1
			Zmax 1
			Phimin -3.141592654
			Phimax 3.141592654
			Triangle_min_angle 3
        }
        Boundary_Conditions {
			R 1 1
			Phi 1 1
			Z 1 1
        }
    }
    Time {
        Time-Step {
            Delta-Time  1e-012
            Type  Automatic
        }
        Time-Window {
            End-Time  6.0049e-007
            Type  User-defined
        }
        Tolerance {
            Decay      -40  // (dB)
            Variation  -30  // (dB)
        }
        Recording-Interval {
            Observer  74
            Snapshot  8
        }
    }
    Method {
        Solver  AUTO
        ADI-PPP  20  // Points Per Period
    }
}

Geometry_v2.0 
{
	[solids]
	[solid]
		Name: "Sphere"
		Material: "NormalMaterial1"
		Mesh: "1"
		Name: "Sphere"
		Transparency: "0"
		[components]

		[ellipsoid]
		Operation Type: "add"
		Name: "Shape1"
		Origin: "0, 0, 0"
		U_Axis: "1, 0, 0"
		V_Axis: "0, 1, 0"
		Ru: "6"
		Rv: "6"
		Rw: "6"
		[end ellipsoid]

		[end components]
	[end solid]

	[end solids]


}

Source
{
    Source1 {
        Type {
            Dipole Electric
            Position  0  0  0  // x,y,z
            Polarization  1  0  0  // Hx,Hy,Hz
        }
        Excitation {
            Amplitude  1
            Delay  0
            Project-Pulse
        }
    }
}

Observer
{
    r1 {
        Component  7
        Position  0  0  4  // x,y,z
    }
    r2 {
        Component  7
        Position  1  0  4  // x,y,z
    }
    r3 {
        Component  7
        Position  2  0  4  // x,y,z
    }
    r4 {
        Component  7
        Position  3  0  4  // x,y,z
    }
    r5 {
        Component  7
        Position  4  0  4  // x,y,z
    }
    r6 {
        Component  7
        Position  5  0  4  // x,y,z
    }
    r7 {
        Component  7
        Position  6  0  4  // x,y,z
    }
    r8 {
        Component  7
        Position  7  0  4  // x,y,z
    }
}

Multi-Domain
{
    Enable
    Input-Method  Position
    Num-Div  1 1 1
    X-Pos { }
    Y-Pos { }
    Z-Pos { }
    Subdomain_solver_type { 0 }
}

Hybrid-Domain
{
    Disable
    Background {
        Type  ECT
        Box   0 0 0   0 0 0
    }
}

Option
{
    Observer-Spectrum  1
    ResultType-ParamAnal 0
}

Comparison-Data
{
}

Parametric-Analysis
{
}

Result-Enable
{
    Source {
        Transient 1
        Spectrum  1
    }
    Observer {
        Transient 1
        Spectrum  1
    }
    Lumped-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  0
        Incident-Voltage-Spectrum   0
        Incident-Current-Transient  0
        Incident-Current-Spectrum   0
        Scattered-Voltage-Transient 0
        Scattered-Voltage-Spectrum  0
        Scattered-Current-Transient 0
        Scattered-Current-Spectrum  0
    }
    Wave-Port {
        S-Parameter                 1
        Impedance                   1
        Incident-Voltage-Transient  0
        Incident-Voltage-Spectrum   0
        Incident-Current-Transient  0
        Incident-Current-Spectrum   0
        Scattered-Voltage-Transient 0
        Scattered-Voltage-Spectrum  0
        Scattered-Current-Transient 0
        Scattered-Current-Spectrum  0
    }
    Spice {
        Voltage-Transient  1
        Voltage-Spectrum   0
        Current-Transient  1
        Current-Spectrum   0
    }
    RLCD {
        Voltage-Transient  1
        Voltage-Spectrum   0
        Current-Transient  1
        Current-Spectrum   0
    }
    Snapshot {
        Enable  0
    }
    Far-Field {
        Enable  0
    }
}

Variable-Sub-System
{
}

Name-System
{
    Body  {
        Name  Body
        Index 1
    }
    Body-Copy  {
        Name  c
        Index 1
    }
    Body-Mirror  {
        Name  m
        Index 1
    }
    Body-Rotate  {
        Name  r
        Index 1
    }
    Body-Trans  {
        Name  t
        Index 1
    }
}

Water-Mark
{
{000292-012382-017421-018716}
}

